Measurement Protocol PAX

# General Information:

|  |  |  |
| --- | --- | --- |
| Test date: 16/9/20 | Date prev. test: 14/9/20 | Test number: 2 |
| Tested by: Sarah Schoultz | PAX number: PB-027 | Installed at ant.: NA |
| Comments: Y PAM taken from PAX 21 X Pol | | |
|  | | |
|  | | |
|  | | |
| Known problems: Bowl shaped Y passband so filter or slope supporter possibly broken | | |
|  | | |
|  | | |
|  | | |

# Setup:

|  |  |  |  |
| --- | --- | --- | --- |
| Power supply: | OK 🗹 NOK 🗆 | Communication: | OK 🗹 NOK 🗆 |
| Supply current +6V: 1.123mA | | ssh obs@antcntl | |
| Supply current -6V: 0.104mA | | ssh ataant@ant0 | pw: q@n@t |
| Supply current +5V: 0.181mA | | telnet pax | “help” |
|  | | CTRL + ] | “close” |

# RF Test with VNA:

### VNA Setup:

|  |  |  |
| --- | --- | --- |
| Load configuration: Passband\_PAX.csa | | |
| Freq Start: 1.0 GHz | Freq Stop: 13.0 GHz | Power Level: -20 dBm |
| Averaging: enabled | Averaging count: 15 | N. Points: 801 |
| VNA : Agilent N5230C 10MHz - 20GHz | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VNA to PAX connection: | 1m ABC-CA18 Cable + 20dB Attenuator | | | |
| Input Power Level to PAX: (Measured) | @1GHz:  -40.2dBm | @4GHz:  -40.7dBm | @8GHz: -41.2dBm | @12GHz: -41.4dBm |

|  |  |
| --- | --- |
| PAX to VNA connection: | 2m Fibre Cable + Fibre Diode + AOX Amplifier + 1m ABC-CA18 Cable |

### Measured Passband with Attenuator set to 7dB each (Complete Link):

|  |
| --- |
| X |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Flatness: | OK 🗆 NOK 🗹 | Unwanted Features: | Yes 🗹 No 🗆 |

|  |
| --- |
| Y |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Flatness: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗆 No 🗹 |

### Power Sweep (Complete Link):

|  |  |  |
| --- | --- | --- |
| Load configuration: Power\_Sweep\_PAX.csa | | |
| Power Start: -40dBm | Power Stop: -20dBm | Frequency : 4.0GHz |
| PAM Attenuator: 0dB |  | N. Points: 801 |

|  |
| --- |
| X |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Compression point: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗆 No 🗹 |

|  |
| --- |
| Y |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Compression point: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗆 No 🗹 |

### Detector Calibration and Attenuator Sweep Pol X:

|  |  |  |
| --- | --- | --- |
| Load configuration: Detector\_Calibration\_PAX.csa | | |
| Freq : 4.0 GHz | Power Level: -20dBm | Sweep Time: -20sec |
| Sweep Mode: CW | Power Level at PAX Input (Measured): -40.6dBm | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| X | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -40.6 | 0 | 0 | - | 12.7 |
| -40.6 | 0 | 3 | - | 12.7 |
| -40.6 | 0 | 6 | - | 11.7 |
| -40.6 | 0 | 9 | - | 9.5 |
| -40.6 | 0 | 12 | 0.8516 | 6.6 |
| -40.6 | 0 | 15 | 0.7523 | 3.8 |
| -40.6 | 0 | 18 | 0.4117 | 0.4 |
| -40.6 | 0 | 21 | 0.2294 | -2.6 |
| -40.6 | 3 | 21 | 0.1155 | -5.9 |
| -40.6 | 6 | 21 | 0.0608 | -8.9 |
| -40.6 | 9 | 21 | 0.0314 | -11.9 |
| -40.6 | 12 | 21 | 0.0165 | -14.9 |
| -40.6 | 15 | 21 | 0.0090 | -17.8 |
| -40.6 | 18 | 21 | 0.0048 | -21.1 |
| -40.6 | 21 | 21 | 0.0029 | -24.2 |
| -40.6 | 24 | 21 | 0.0020 | -27.0 |
| -40.6 | 27 | 21 | 0.0015 | -30.0 |
| -40.6 | 30 | 21 | 0.0013 | -33.2 |
| -40.6 | 30 | 24 | 0.0012 | -35.8 |
| -40.6 | 30 | 27 | 0.0011 | -38.3 |
| -40.6 | 30 | 30 | 0.0011 | -40.7 |

|  |  |  |
| --- | --- | --- |
| Use Noise Source: Atlantic AS6333 | | |
| Freq : 1.0 - 12.0GHz | Power Level: -41.8dBm |  |
| DC Supply: 28V |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| X | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -41.8 | 0 | 0 | - | 11.2 |
| -41.8 | 0 | 3 | - | 10.2 |
| -41.8 | 0 | 6 | - | 8.6 |
| -41.8 | 0 | 9 | - | 6.7 |
| -41.8 | 0 | 12 | 0.8510 | 4.0 |
| -41.8 | 0 | 15 | 0.7779 | 1.5 |
| -41.8 | 0 | 18 | 0.4201 | -1.7 |
| -41.8 | 0 | 21 | 0.2302 | -4.6 |
| -41.8 | 3 | 21 | 0.1193 | -7.5 |
| -41.8 | 6 | 21 | 0.0594 | -10.6 |
| -41.8 | 9 | 21 | 0.0308 | -13.5 |
| -41.8 | 12 | 21 | 0.0158 | -16.5 |
| -41.8 | 15 | 21 | 0.0091 | -19.2 |
| -41.8 | 18 | 21 | 0.0049 | -22.5 |
| -41.8 | 21 | 21 | 0.0031 | -25.6 |
| -41.8 | 24 | 21 | 0.0022 | -28.6 |
| -41.8 | 27 | 21 | 0.0019 | -31.3 |
| -41.8 | 30 | 21 | 0.0016 | -34.5 |
| -41.8 | 30 | 24 | 0.0015 | -37.1 |
| -41.8 | 30 | 27 | 0.0014 | -39.3 |
| -41.8 | 30 | 30 | 0.0015 | -41.4 |

### Detector Calibration and Attenuator Sweep Pol Y:

|  |  |  |
| --- | --- | --- |
| Load configuration: Detector\_Calibration\_PAX.csa | | |
| Freq : 4.0 GHz | Power Level: -20dBm | Sweep Time: -20sec |
| Sweep Mode: CW | Power Level at PAX Input (Measured): -40.6dBm | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Y | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -40.6 | 0 | 0 | - | 10.0 |
| -40.6 | 0 | 3 | 0.8489 | 7.7 |
| -40.6 | 0 | 6 | 0.7595 | 5.0 |
| -40.6 | 0 | 9 | 0.4855 | 2.2 |
| -40.6 | 0 | 12 | 0.2922 | -0.8 |
| -40.6 | 0 | 15 | 0.1731 | -3.7 |
| -40.6 | 0 | 18 | 0.0863 | -7.2 |
| -40.6 | 0 | 21 | 0.0482 | -10.1 |
| -40.6 | 3 | 21 | 0.0237 | -13.4 |
| -40.6 | 6 | 21 | 0.0124 | -16.3 |
| -40.6 | 9 | 21 | 0.0065 | -19.4 |
| -40.6 | 12 | 21 | 0.0037 | -22.4 |
| -40.6 | 15 | 21 | 0.0023 | -25.3 |
| -40.6 | 18 | 21 | 0.0015 | -28.6 |
| -40.6 | 21 | 21 | 0.0011 | -31.7 |
| -40.6 | 24 | 21 | 0.0009 | -34.6 |
| -40.6 | 27 | 21 | 0.0009 | -37.5 |
| -40.6 | 30 | 21 | 0.0008 | -40.5 |
| -40.6 | 30 | 24 | 0.0008 | -42.6 |
| -40.6 | 30 | 27 | 0.0008 | -44.6 |
| -40.6 | 30 | 30 | 0.0007 | -46.2 |

|  |  |  |
| --- | --- | --- |
| Use Noise Source: Atlantic AS6333 | | |
| Freq : 1.0 - 12.0GHz | Power Level: -41.8dBm |  |
| DC Supply: 28V |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Y | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -41.8 | 0 | 0 | - | 7.0 |
| -41.8 | 0 | 3 | 0.8484 | 5.1 |
| -41.8 | 0 | 6 | 0.7965 | 2.8 |
| -41.8 | 0 | 9 | 0.5364 | 0.3 |
| -41.8 | 0 | 12 | 0.3206 | -2.7 |
| -41.8 | 0 | 15 | 0.2043 | -5.2 |
| -41.8 | 0 | 18 | 0.0977 | -8.7 |
| -41.8 | 0 | 21 | 0.0532 | -11.4 |
| -41.8 | 3 | 21 | 0.0267 | -14.5 |
| -41.8 | 6 | 21 | 0.0135 | -17.5 |
| -41.8 | 9 | 21 | 0.0074 | -20.3 |
| -41.8 | 12 | 21 | 0.0042 | -23.4 |
| -41.8 | 15 | 21 | 0.0027 | -26.2 |
| -41.8 | 18 | 21 | 0.0018 | -29.4 |
| -41.8 | 21 | 21 | 0.0015 | -32.3 |
| -41.8 | 24 | 21 | 0.0013 | -35.5 |
| -41.8 | 27 | 21 | 0.0012 | -38.2 |
| -41.8 | 30 | 21 | 0.0012 | -41.3 |
| -41.8 | 30 | 24 | 0.0011 | -43.4 |
| -41.8 | 30 | 27 | 0.0010 | -45.0 |
| -41.8 | 30 | 30 | 0.0011 | -46.5 |

# Inspection:

### Visual:

|  |  |  |
| --- | --- | --- |
| Fibre Connectors Clean | Comments: | OK 🗹 NOK 🗆 |
| Fibre Connector Mechanical | Comments: | OK **🗹** NOK **🗆** |
| RF Cable | Comments: | OK **🗹** NOK **🗆** |
| RF Connectors Clean | Comments: | OK **🗹** NOK **🗆** |
| RF Connector on PAM screws tight | Comments: | OK **🗹** NOK **🗆** |

### Functions:

|  |  |  |
| --- | --- | --- |
| Read Temperature Value | Comments: 29.1 | OK 🗹 NOK 🗆 |
| LNA Settings | Comments: | OK 🗆 NOK **🗆** |
| Temperature Stabilisation | Comments: | OK 🗆 NOK **🗆** |