Measurement Protocol PAX

# General Information:

|  |  |  |
| --- | --- | --- |
| Test date: 11/9/20 | Date prev. test: NA | Test number: 1 |
| Tested by: Sarah Schoultz | PAX number: PB-042 | Installed at ant.: NA |
| Comments: | | |
|  | | |
|  | | |
|  | | |
| Known problems: | | |
|  | | |
|  | | |
|  | | |

# Setup:

|  |  |  |  |
| --- | --- | --- | --- |
| Power supply: | OK 🗹 NOK 🗆 | Communication: | OK 🗹 NOK 🗆 |
| Supply current +6V: 1.109mA | | ssh obs@antcntl | |
| Supply current -6V: 0.123mA | | ssh ataant@ant0 | pw: q@n@t |
| Supply current +5V: 0.157mA | | telnet pax | “help” |
|  | | CTRL + ] | “close” |

# RF Test with VNA:

### VNA Setup:

|  |  |  |
| --- | --- | --- |
| Load configuration: Passband\_PAX.csa | | |
| Freq Start: 1.0 GHz | Freq Stop: 13.0 GHz | Power Level: -20 dBm |
| Averaging: enabled | Averaging count: 15 | N. Points: 801 |
| VNA : Agilent N5230C 10MHz - 20GHz | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VNA to PAX connection: | 1m ABC-CA18 Cable + 20dB Attenuator | | | |
| Input Power Level to PAX: (Measured) | @1GHz:  -40.2dBm | @4GHz:  -40.7dBm | @8GHz: -41.2dBm | @12GHz: -41.4dBm |

|  |  |
| --- | --- |
| PAX to VNA connection: | 2m Fibre Cable + Fibre Diode + AOX Amplifier + 1m ABC-CA18 Cable |

### Measured Passband with Attenuator set to 7dB each (Complete Link):

|  |
| --- |
| X |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Flatness: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗆 No 🗹 |

|  |
| --- |
| Y |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Flatness: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗹 No 🗆 |

### Power Sweep (Complete Link):

|  |  |  |
| --- | --- | --- |
| Load configuration: Power\_Sweep\_PAX.csa | | |
| Power Start: -40dBm | Power Stop: -20dBm | Frequency : 4.0GHz |
| PAM Attenuator: 0dB |  | N. Points: 801 |

|  |
| --- |
| X |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Compression point: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗆 No 🗹 |

|  |
| --- |
| Y |

A screenshot of a cell phone

Description automatically generated

|  |  |  |  |
| --- | --- | --- | --- |
| Compression point: | OK 🗹 NOK 🗆 | Unwanted Features: | Yes 🗹 No 🗆 |

### Detector Calibration and Attenuator Sweep Pol X:

|  |  |  |
| --- | --- | --- |
| Load configuration: Detector\_Calibration\_PAX.csa | | |
| Freq : 4.0 GHz | Power Level: -20dBm | Sweep Time: -20sec |
| Sweep Mode: CW | Power Level at PAX Input (Measured): -40.6dBm | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| X | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -40.6 | 0 | 0 | - | 12.7 |
| -40.6 | 0 | 3 | - | 12.6 |
| -40.6 | 0 | 6 | - | 11.8 |
| -40.6 | 0 | 9 | 0.8327 | 9.8 |
| -40.6 | 0 | 12 | 0.7842 | 6.9 |
| -40.6 | 0 | 15 | 0.5148 | 4.1 |
| -40.6 | 0 | 18 | 0.3038 | 0.9 |
| -40.6 | 0 | 21 | 0.1802 | -2.2 |
| -40.6 | 3 | 21 | 0.0958 | -5.6 |
| -40.6 | 6 | 21 | 0.0521 | -8.6 |
| -40.6 | 9 | 21 | 0.0280 | -11.6 |
| -40.6 | 12 | 21 | 0.0147 | -14.6 |
| -40.6 | 15 | 21 | 0.0079 | -17.6 |
| -40.6 | 18 | 21 | 0.0042 | -20.9 |
| -40.6 | 21 | 21 | 0.0023 | -24.0 |
| -40.6 | 24 | 21 | 0.0016 | -26.8 |
| -40.6 | 27 | 21 | 0.0011 | -29.9 |
| -40.6 | 30 | 21 | 0.0009 | -33.1 |
| -40.6 | 30 | 24 | 0.0008 | -35.7 |
| -40.6 | 30 | 27 | 0.0007 | -38.2 |
| -40.6 | 30 | 30 | 0.0007 | -40.6 |

|  |  |  |
| --- | --- | --- |
| Use Noise Source: Atlantic AS6333 | | |
| Freq : 1.0 - 12.0GHz | Power Level: -41.8dBm |  |
| DC Supply: 28V |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| X | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -41.8 | 0 | 0 | - | 11.1 |
| -41.8 | 0 | 3 | - | 10.1 |
| -41.8 | 0 | 6 | - | 8.6 |
| -41.8 | 0 | 9 | 0.8334 | 6.6 |
| -41.8 | 0 | 12 | 0.6905 | 4.0 |
| -41.8 | 0 | 15 | 0.4634 | 1.5 |
| -41.8 | 0 | 18 | 0.2680 | -1.7 |
| -41.8 | 0 | 21 | 0.1563 | -4.6 |
| -41.8 | 3 | 21 | 0.0857 | -7.6 |
| -41.8 | 6 | 21 | 0.0442 | -10.8 |
| -41.8 | 9 | 21 | 0.0237 | -13.6 |
| -41.8 | 12 | 21 | 0.0122 | -16.7 |
| -41.8 | 15 | 21 | 0.0070 | -19.3 |
| -41.8 | 18 | 21 | 0.0038 | -22.7 |
| -41.8 | 21 | 21 | 0.0024 | -25.7 |
| -41.8 | 24 | 21 | 0.0017 | -28.7 |
| -41.8 | 27 | 21 | 0.0014 | -31.4 |
| -41.8 | 30 | 21 | 0.0011 | -34.7 |
| -41.8 | 30 | 24 | 0.0011 | -37.3 |
| -41.8 | 30 | 27 | 0.0010 | -39.4 |
| -41.8 | 30 | 30 | 0.0010 | -41.5 |

### Detector Calibration and Attenuator Sweep Pol Y:

|  |  |  |
| --- | --- | --- |
| Load configuration: Detector\_Calibration\_PAX.csa | | |
| Freq : 4.0 GHz | Power Level: -20dBm | Sweep Time: -20sec |
| Sweep Mode: CW | Power Level at PAX Input (Measured): -40.6dBm | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Y | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -40.6 | 0 | 0 | - | 14.0 |
| -40.6 | 0 | 3 | - | 14.0 |
| -40.6 | 0 | 6 | - | 13.3 |
| -40.6 | 0 | 9 | - | 11.1 |
| -40.6 | 0 | 12 | 0.8589 | 8.2 |
| -40.6 | 0 | 15 | 0.6506 | 5.4 |
| -40.6 | 0 | 18 | 0.3425 | 2.0 |
| -40.6 | 0 | 21 | 0.1844 | -1.1 |
| -40.6 | 3 | 21 | 0.0891 | -4.4 |
| -40.6 | 6 | 21 | 0.0437 | -7.6 |
| -40.6 | 9 | 21 | 0.0217 | -10.8 |
| -40.6 | 12 | 21 | 0.0110 | -14.0 |
| -40.6 | 15 | 21 | 0.0060 | -17.1 |
| -40.6 | 18 | 21 | 0.0032 | -20.7 |
| -40.6 | 21 | 21 | 0.0021 | -24.0 |
| -40.6 | 24 | 21 | 0.0016 | -27.1 |
| -40.6 | 27 | 21 | 0.0013 | -30.3 |
| -40.6 | 30 | 21 | 0.0012 | -33.7 |
| -40.6 | 30 | 24 | 0.0011 | -36.3 |
| -40.6 | 30 | 27 | 0.0012 | -38.7 |
| -40.6 | 30 | 30 | 0.0011 | -41.0 |

|  |  |  |
| --- | --- | --- |
| Use Noise Source: Atlantic AS6333 | | |
| Freq : 1.0 - 12.0GHz | Power Level: -41.8dBm |  |
| DC Supply: 28V |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Y | | | | |
| CW Input Power [dBm]: | Attenuator Value A [dB]: | Attenuator Value: B [dB]: | Detector Value: | Power Meter  Value [dBm]: |
| -41.8 | 0 | 0 | - | 12.6 |
| -41.8 | 0 | 3 | - | 11.6 |
| -41.8 | 0 | 6 | - | 10.0 |
| -41.8 | 0 | 9 | - | 8.0 |
| -41.8 | 0 | 12 | 0.8584 | 5.3 |
| -41.8 | 0 | 15 | 0.6297 | 2.8 |
| -41.8 | 0 | 18 | 0.3283 | -0.4 |
| -41.8 | 0 | 21 | 0.1773 | -3.4 |
| -41.8 | 3 | 21 | 0.0942 | -6.4 |
| -41.8 | 6 | 21 | 0.0449 | -9.7 |
| -41.8 | 9 | 21 | 0.0230 | -12.8 |
| -41.8 | 12 | 21 | 0.0113 | -16.0 |
| -41.8 | 15 | 21 | 0.0068 | -18.8 |
| -41.8 | 18 | 21 | 0.0037 | -22.6 |
| -41.8 | 21 | 21 | 0.0025 | -25.9 |
| -41.8 | 24 | 21 | 0.0019 | -29.2 |
| -41.8 | 27 | 21 | 0.0016 | -32.1 |
| -41.8 | 30 | 21 | 0.0015 | -35.6 |
| -41.8 | 30 | 24 | 0.0014 | -38.1 |
| -41.8 | 30 | 27 | 0.0015 | -40.2 |
| -41.8 | 30 | 30 | 0.0014 | -42.1 |

# Inspection:

### Visual:

|  |  |  |
| --- | --- | --- |
| Fibre Connectors Clean | Comments: | OK 🗹 NOK 🗆 |
| Fibre Connector Mechanical | Comments: | OK **🗹** NOK **🗆** |
| RF Cable | Comments: | OK **🗹** NOK **🗆** |
| RF Connectors Clean | Comments: | OK **🗹** NOK **🗆** |
| RF Connector on PAM screws tight | Comments: | OK **🗹** NOK **🗆** |

### Functions:

|  |  |  |
| --- | --- | --- |
| Read Temperature Value | Comments: 31.6 | OK 🗹 NOK 🗆 |
| LNA Settings | Comments: | OK 🗆 NOK **🗆** |
| Temperature Stabilisation | Comments: | OK 🗆 NOK **🗆** |