# This document describes how to set the MAC address in the DHCP server at control.hcro.org after a controlbox swap.

## Intro:

Connect to control as ROOT “ssh root@control”

nano /etc/dhcp/dhcpd.ataants.conf

systemctl restart isc-dhcp-server.service

## Important:

To check what is on the antenna network run:

arp -i ens2f3