# This document describes how to configure the BBB to boot from SD card.

## Intro:

This is required using a new BBB.

Mount boot partition and overwrite it

https://fastbitlab.com/linux-device-driver-lecture-10-making-sd-boot-default-on-bbb-by-erasing-emmc-mbr/